{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["CK报警","监控"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CK报警","index":0,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["附件：\n                    报 警 器 材"]
["序\n号","设备名称","规格、型号","品牌"]
[1,"238plusII主机、键盘","238plusII","Honeywell"]
[2,"2316plusI主机键盘","2316plusII","Honeywell"]
[3,"紧急按钮","pb-2","Honeywell"]
[4,"振动探测器","ISC-SK10-CHI","BOSCH"]
[5,"声光警号","HC-102","豪恩"]
[6,"声光警号","kt-g500","KEST"]
[7,"线材4*0.5","线材4*0.5"]
[8,"无线模块","WT-300T","BOSCH"]
[9,"无线模块","MC-37I","Think"]
[10,"探测器","EAGLE-DT","EL"]
[11,"蓄电池",1270,"统一"]
[12,"探测器","WP12G","BOSCH"]
[13,"网络4防区报警主机","COMPACT-4","Honeywell"]
[14,"支架","万向"]
[15,"探测器","WP15G","BOSCH"]
[16,"探测器","DT8035","Honeywell"]

{"sheet":"监控","index":1,"n_rows":170,"n_cols":5,"rows_kept":170,"merged":[[0,0,0,4],[2,0,13,0],[14,0,27,0],[28,0,41,0],[42,0,55,0],[56,0,57,0],[58,0,69,0],[70,0,76,0],[77,0,83,0],[84,0,94,0],[95,0,97,0],[98,0,111,0],[112,0,124,0],[126,0,139,0],[140,0,153,0],[154,0,155,0],[159,0,167,0],[168,0,169,0]],"flags":["formulas_cached_only"]}
["附件：\n                              器 材 清 单"]
["分项","序号","设备名称","规格、型号","品牌"]
["\n\n\n\n\n1、监控设备",1,"摄像机","DS-2CD3345FD-I","海康"]
[null,2,"摄像机","DS-2CD3345F-I","海康"]
[null,3,"摄像机","DS-2CD3345F-IS","海康"]
[null,4,"摄像机","DS-2CD3T35D-I3","海康"]
[null,5,"摄像机","DS-2CD3T35-I3","海康"]
[null,6,"摄像机","DS-2CD3T35D-I5","海康"]
[null,7,"摄像机","DS-2CD3T35-I5","海康"]
[null,8,"摄像机","DS-2CD3T35-I8","海康"]
[null,9,"摄像机","DS-2CD3T35D-I8","海康"]
[null,10,"摄像机","DS-2DC7320IW-A","海康"]
[null,11,"摄像机","DS-2DC7220IW-A","海康"]
[null,12,"摄像机","DS-2DC7120IW-A","海康"]
["监控设备",13,"硬盘录像机","DS-7804N-K1","海康"]
[null,14,"硬盘录像机","DS-7908N-K4","海康"]
[null,15,"硬盘录像机","DS-7916N-K4","海康"]
[null,16,"硬盘录像机","DS-7932N-K4","海康"]
[null,17,"硬盘录像机","DS-7908N-K4/8P","海康"]
[null,18,"硬盘录像机","DS-7916N-K4/16P","海康"]
[null,19,"硬盘录像机","DS-7932N-K4/16P","海康"]
[null,20,"西数1T监控盘","WD10PURX","海康"]
[null,21,"西数2T监控盘","WD20PURX","海康"]
[null,22,"西数3T监控盘","WD30PURX","海康"]
[null,23,"西数4T监控盘","WD40PURX","海康"]
[null,24,"西数6T监控盘","WD60PURX","海康"]
[null,25,"支架","铝合金 大鸭嘴","定制"]
[null,26,"12V电源","2A","小耳朵"]
["2、报警器材",27,"12V电源","10A","小耳朵"]
[null,28,"12V电源","20A","小耳朵"]
[null,29,"24V","100VA","德力西"]
[null,30,"24V","200VA","德力西"]
[null,31,"视频光端机","单路 反向数据","新创"]
[null,32,"液晶电视吊架","NBT560-15","NB"]
[null,33,"液晶电视挂架","NBC3-F","NB"]
[null,34,"室外防水箱","304不锈钢","定制"]
[null,35,"室内防水箱","喷塑","定制"]
[null,1,"大型总线制报警主机","FC-7448","FOCUS"]
[null,2,"家用报警主机","FC-300","FOCUS"]
[null,3,"工程报警主机","FC-7668","FOCUS"]
[null,4,"红外微波双鉴报警探测器","DT-7425","FOCUS"]
[null,5,"红外微波双鉴报警探测器","DT-700","FOCUS"]
["报警器材",6,"无线红外微波双鉴报警\n探测器","DT-55R","FOCUS"]
[null,7,"红外微波双鉴幕帘","DDP-968","FOCUS"]
[null,8,"门磁","MD-209R","FOCUS"]
[null,9,"三光束红外对射","ABE-100","FOCUS"]
[null,10,"双防区电子围栏脉冲主机","G5S211","广拓（上海）"]
[null,11,"单防区电子围栏脉冲主机","G5S111","广拓（上海）"]
[null,12,"双防区电子围栏感应主机","T6211","广拓（上海）"]
[null,13,"单防区电子围栏感应主机","T6111","广拓（上海）"]
[null,14,"张力控制器","V5","广拓（上海）"]
[null,15,"双防区张力控制杆","ZL-KZG4-AL04","广拓（上海）"]
[null,16,"单防区张力控制杆","ZL-KZG4-AL03","广拓（上海）"]
[null,17,"电子围栏","4线制","广拓（上海）"]
[null,18,"张力电子围栏","4线制","广拓（上海）"]
[null,19,"电子围栏防水箱","FYX-V5-01","广拓（上海）"]
["报警器材",20,"电子围栏防雷器","HWH","广拓（上海）"]
[null,21,"电子围栏智能控制键盘","MK200","广拓（上海）"]
["3、显示存储设备",1,"2T企业级硬盘","WD2003FZEX","西数"]
[null,2,"3T企业级硬盘","WD3003FZEX","西数"]
[null,3,"2T服务器硬盘"," 7.2K RPM SAS 6Gbps","DELL"]
[null,4,"显示器 21寸","S22F350FH","三星"]
[null,5,"显示器 23寸","S24D360HL","三星"]
[null,6,"显示器 21寸","226V6QSB6","飞利浦"]
[null,7,"显示器 23寸"," 233E4QSD","飞利浦"]
[null,8,"显示器 21寸","E2252SWDN","AOC"]
[null,9,"显示器 23寸","P2491VWHE/BW","AOC"]
[null,10,"液晶电视机 32寸","32PHF5055/T3","飞利浦"]
[null,11,"液晶电视机 40寸","40PFF5650/T3","飞利浦"]
[null,12,"液晶电视机 50寸","50PFF5655/T3","飞利浦"]
["显示存储设备",13,"液晶电视机 58寸","58PFF3250/T3","飞利浦"]
[null,14,"液晶电视机 65寸","65PUF6059/T3 ","飞利浦"]
[null,15,"液晶电视机 32寸","LCD-32M3A","夏普"]
[null,16,"液晶电视机 40寸","LCD-40M3A","夏普"]
[null,17,"液晶电视机 50寸","LCD-50S3A","夏普"]
[null,18,"液晶电视机 60寸","LCD-60UF30A","夏普"]
[null,19,"液晶电视机 65寸","LCD-65S3A","夏普"]
["4、H3C DLINK网络设备",1,"24口千兆POE交换机","S5120-28P-POE-Winet","H3C"]
[null,2,"24口百兆POE交换机","SMB-S2626-PWR","H3C"]
[null,3,"8口千兆POE交换机","S1208-PWR","H3C"]
[null,4,"48+4口千兆交换机","S5120-52P-LI ","H3C"]
[null,5,"48口千兆交换机","SMB-S1824G","H3C"]
[null,6,"48口百兆交换机","S1048","H3C"]
[null,7,"48口百兆交换机","S1550","H3C"]
["H3C DLINK网络设备",8,"24口全千兆交换机","S5700-24TP-SI-AC ","H3C"]
[null,9,"24口全千兆交换机","S5120-28P-LI","H3C"]
[null,10,"24口全千兆交换机"," S1224RV2 ","H3C"]
[null,11,"24口百兆交换机","S1026T","H3C"]
[null,12,"24口百兆交换机","S1024","H3C"]
[null,13,"16口百兆交换机","S1016R","H3C"]
[null,14,"无线AP","EWP-WA2620-AGN-C","H3C"]
[null,15,"无线AP","EWP-WAP621","H3C"]
[null,16,"光纤收发模块","SFP-GE-LX-SM1310-D","H3C"]
[null,17,"无线路由器","DIR-629","DLINK"]
[null,18,"光纤千兆收发器","DGE-872","DLINK"]
["5、TPLINK网络设备",1,"光纤百兆收发器","TR-962D ","TP LINK"]
[null,2,"5口POE交换机","SF1005P","TP LINK"]
[null,3,"9口POE交换机","SF1009PE","TP LINK"]
["5、TPLINK网络设备",4,"16口POE交换机","SL1218P","TP LINK"]
[null,5,"24口POE交换机","SL1226PE","TP LINK"]
[null,6,"无线网桥","TLCPE510","TP LINK"]
[null,7,"无线网桥","TLBS510+TL-ANT5819MS","TP LINK"]
[null,8,"无线网桥","TLBS510+TL-ANT5830MD","TP LINK"]
[null,9,"无线网桥","NanoStationM5 NSM5 airMAX\n 5GHz","UBNT"]
[null,10,"无线网桥","UniFi UAP-Outdoor+","UBNT"]
[null,11,"无线网桥","airFiber AF-5X 5GHz","UBNT"]
[null,12,"机柜","前玻后网600×800×2000","图腾(中国)"]
[null,13,"机柜","前玻后网600×800×1200","图腾(中国)"]
[null,14,"机柜","前玻后网600×800×2000","普通"]
[null,15,"机柜","前玻后网600×800×1200","普通"]
[null,16,"ODF","72芯","定制"]
[null,17,"ODF","48芯","定制"]
["5、TPLINK网络设备",18,"光纤终端盒","机架式12芯","中天"]
[null,19,"光纤终端盒","4芯","中天"]
[null,20,"光纤熔接包","4出线口","中天"]
[null,21,"光纤跳线","LC-LC 3M","LINK"]
[null,22,"光纤跳线","FC-FC 3M","LINK"]
[null,23,"语音配线架100对","PI3100","TCL"]
[null,24,"6类配线架",632781,"TCL"]
[null,25,"超5类配线架","PD1124-11","TCL"]
[null,26,"理线架","PA3211(02)","TCL"]
[null,27,"6类网络模块","PM2013","TCL"]
[null,28,"超5类网络模块","PM1011","TCL"]
[null,29,"超5类水晶头","4-554720-3 ","TCL"]
[null,30,"6类水晶头","6-2111979-3","TCL"]
["6、线缆",1,"电源线","RVV2×1.5","视通"]
["6、线缆",2,"电源线","RVV2×2.0","视通"]
[null,3,"电源线","RVV2×2.5","视通"]
[null,4,"电源线","RVV4×0.75","视通"]
[null,5,"电源线","RVV4×1.0","视通"]
[null,6,"电源线","RVV2×1.0","天诚"]
[null,7,"电源线","RVV2×1.5","天诚"]
[null,8,"电源线","RVV2×2.0","天诚"]
[null,9,"电源线","RVV2×2.5","天诚"]
[null,10,"电源线","RVV4×0.75","天诚"]
[null,11,"电源线","RVV4×1.0","天诚"]
[null,12,"超5类网线",null,"TCL"]
[null,13,"超5类防水网线",null,"TCL"]
[null,14,"6类网线",null,"TCL"]
[null,15,"6类防水网线",null,"TCL"]
["6、线缆",16,"超5类网线",null,"DLINK"]
[null,17,"超5类防水网线",null,"DLINK"]
[null,18,"6类网线",null,"DLINK"]
[null,19,"6类防水网线",null,"DLINK"]
[null,20,"超5类网线",null,"视通"]
[null,21,"超5类防水网线",null,"视通"]
[null,22,"6类网线",null,"视通"]
[null,23,"6类防水网线",null,"视通"]
[null,24,"光纤","单模8芯","中天(中国)"]
[null,25,"光纤","单模12芯","中天(中国)"]
[null,26,"光纤","单模24芯","中天(中国)"]
[null,27,"光纤","单模48芯","中天(中国)"]
[null,28,"光纤","单模8芯","视通"]
[null,29,"光纤","单模12芯","视通"]
["6、线缆",30,"光纤","单模24芯","视通"]
[null,31,"光纤","单模48芯","视通"]
["7、管材桥架",1,"pvc管","φ16","三德（新加坡）"]
[null,2,"pvc管","φ20","三德（新加坡）"]
[null,3,"pvc管","φ25","三德（新加坡）"]
["7、管材桥架",4,"JDG","φ20","国标"]
[null,5,"JDG","φ25","国标"]
[null,6,"热镀锌钢管","DN20","国标"]
[null,7,"热镀锌钢管","DN25","国标"]
[null,8,"热镀锌钢管","DN50","国标"]
[null,9,"尼龙管",null,"国标"]
[null,10,"桥架","镀锌喷塑50×100含托架配件","国标"]
[null,11,"桥架","镀锌喷塑50×150含托架配件","国标"]
[null,12,"桥架","镀锌喷塑100×150含托架配件","国标"]
["7、管材桥架",13,"桥架","镀锌喷塑100×200含托架配件","国标"]
[null,14,"桥架","镀锌喷塑100×300含托架配件","国标"]